=============================================
[version 2.45.03]

Data = 2007/10/15
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version =
1. Support 8226 HDCP download.
2. 8226_dir,RISC Dram and RISC Reg address inc/dec, 4 bytes jump one time.
3. Use new protocol of 8226 EEPROM R/W.
4. Support 8226 ShareInfo R/W in Dram(Byte) Read Button.
5. Support a new flash AMIC(A25L16P).
6. Support 8202/8226 R/W 4k EEPROM.
7. Support 8202/8226 dump 4k EEPROM.
8. Customize the chip selection to avoid mistake in client service side.
9. Reset 8226 platform in advance before download.
=============================================
[version 2.45.02]

Data = 2007/09/10
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version =
1. Add I2C Device reg type in 8226 reginster R/W window.
=============================================
[version 2.45.01]

Data = 2007/09/07
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version = 
1. Replace I2C Device with EEPROM in reg type of 8226 register R/W window.
=============================================
[version 2.45.00]

Data = 2007/09/06
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version = 
1. Check sum to verify when download F/E binary.
2. Add DSP windows to R/W DSP.
3. Support download/upload 8226 eeprom data.
4. Adjust UI.
=============================================
[version 2.44.05]

Data = 2007/08/24
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version = 
1. flashinf.ini modified. 
2. speed 538x download. 
=============================================
[version 2.44.04]

Data = 2007/07/13
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version = 
1. Support 8MB flash read/write for 8226
2. fixed Fast Dump from file to dram
3. fix ADSP DRAM read/write function not work

ClearCase baseline: 
=============================================
[version 2.44.03]

Data = 2007/06/27
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version = 
1. add PQ Setting page for 538x
2. modify reset button as ncstool (switch its function between connection and disconnection)
3. fix Dram (byte & dword) +/- step error with chip_8226 selected

ClearCase baseline: 
=============================================
[version 2.44.02]

Data = 2007/06/15
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version = 
1. support 8226 serial flash update
2. fix bug of read/write 8226 i2c register
3. support PQ bin partial update for 538x
4. support writing EDID for 538x
5. merge modification for 1379
6. add a button "OK" to show connecting status

ClearCase baseline: 
=============================================
[version 2.44.01]

Data = 2007/5/25
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version = 
1,Support 8226 platform 
2,Support 538x platform 
3,Support 8226_dir data type and GetPC function for 8226 
4,Add EEPROM dump/load function for 537x platform 
5,Release EEPROM dump/load function to customers for 537x platform 
6,Support new flash type F49L160UA/F49L160BA 
7,Fix the AutoTest function in Register R/W form
8,Fix bug of write HDCP 

ClearCase baseline: 
=============================================
[version 2.43.22]

Data = 2007/3/23
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version = 
1. Support blank-checking after flash erased in upgrade process

ClearCase baseline: 
=============================================
[version 2.43.21]

Data = 2007/2/13
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version = 
1. Support flash SST39VF1681

ClearCase baseline: MTKTOOL_00000029
=============================================
[version 2.43.20]

Data = 2007/1/30
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version = 
1. Added function to use the same serial comport with other tool.
2. Fixed bug to backup 537X's flash.
3. Support multi upgrading.
4. Added function to avoid the overlap between the servo binary and 

ClearCase baseline: MTKTOOL_00000028
=============================================
[version 2.43.16]

Data = 2007/1/03
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version = 
1. Show the usless data in ASCII and hex.
2. fix the multi upgrading.
3. Add function to save the MT537X flash's contents as a binary file.
4. Added delay time when MTKTool send data to MT1389

ClearCase baseline: MTKTOOL_00000027
=============================================
[version 2.43.15]

Data = 2006/12/21
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version = 
1. Dump EEPROM to the selected file.
2. Load the selected file to EEPROM.

ClearCase baseline: MTKTOOL_00000026
=============================================
[version 2.43.13]

Data = 2006/11/24
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version = 
1. fixed the bug that writing command's format is wrong.

ClearCase baseline: MTKTOOL_00000024
=============================================
[version 2.43.12]

Data = 2006/11/24
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version = 
1. Speeded up the HDCP key downloading

ClearCase baseline: MTKTOOL_00000023
=============================================
[version 2.43.11]

Data = 2006/11/20
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version = 
1. Added function to support HDCP Key download Under MT537X.
2. Added function to show all received data in log window.
3. Added register type --- I2C (EXTEND)

ClearCase baseline: MTKTOOL_00000022
=============================================
[version 2.43.10]

Data = 2006/11/07
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version = 
1. adjust the delay time length to finish power off.

ClearCase baseline: MTKTOOL_00000021
=============================================
[version 2.43.09]

Data = 2006/09/26
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version = 
1. speedup upgrading HDCP Key under MT537X

ClearCase baseline: MTKTOOL_00000019
=============================================
[version 2.43.08]

Data = 2006/09/19
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version = 
1. config.ini set hdcp key's position.

ClearCase baseline: MTKTOOL_00000019
=============================================
[version 2.43.07]

Data = 2006/09/15
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version = 
1. Scan the little tool when running MTKTool.
2. Run the little tool or the help file.
3. No password, Under MT8105/8158, turn on upgrade HDCP Key function.
4. fix a little bug.

ClearCase baseline: MTKTOOL_00000019
=============================================
[version 2.43.05]

Data = 2006/09/04
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version = 
1. Add function to verify HDCP Key under MT537X.
2. Add function to upgrade serial flash under MT1389.

ClearCase baseline: MTKTOOL_00000018
=============================================
[version 2.43.04]

Data = 2006/08/28
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version = 
1. reset click befroe upgrading.
2. under MT8202, shorten the delay time between the command.
3. Add function to backup/restore the power curve
4. send the command which is saved in file.
5. fix bug -- erase the power curve when upgrading backend firmware.
6. Add register type: IND/DAC
7. Add function to upgrade "HDCP Key" in flash.

ClearCase baseline: MTKTOOL_00000017

=============================================
[version 2.43.02]

Data = 2006/08/11
Owner = Jin Ke

Entry = U:\Hefei\Tools\new\mtktool

Difference from previous version = 
1. Before upgrading process, send command to stop the firmware of 8202 board.
2. Add function to verify the HDCP Key of 8202 board.

ClearCase baseline: MTKTOOL_00000016
