	// WP Pin Share to GPIO
	   rtd_maskl(0xb800180c, 0xffffff0f, 0x50);	
	// Set WP Pin to Output   
		 rtd_maskl(0xb8011208, 0xefffffff, 0x10000000);
	// Set WP Pin to High	 
		 rtd_maskl(0xb801120c, 0xffefffff, 0x100000);
