5 Watts FM-broadcast (87.5-108MHz) transmitter, model: 'Stentor' (Old Dutch design)

All component values are drawn on the .comp and .silklayer bitmaps, with the following
exception(s);

1.- to vary the frequency (+/- 4MHz) mount a variable resistor (100k-Ohms, lineair) at the
    solder points indicated on the drawings.

Notes

(*) not used
CuAg = silver plated copper wire
CuL = magnetwire, enameled copper wire
(Note: 1 mm CuL approx. equals to AWG18
         0,3 mm approx. equals to AWG28)

(I)   all diameters are measured from the inside of the coils
(II)  all coils are air-types and have a wirespacing of approx. 1mm
(III) scrape off the enamel from the wire when soldering the taps on the coils!

Example: 4,5x8x1mm means; 4.5 turns, 8 mm internal coil diameter and 1 mm diameter wire.

A final word of caution, this transmitter has to be fitted with a (good) lowpass filter
between the rf-output and the antenna!

(C)2006 Helix Inc. The Netherlands.

