 Note:
 ====

 The layout of the 2SC1946 28 Watts FM-broadcast RF-amplifier has been created with sPRINT 
 Layout v3.0. You can get a Shareware copy at: http://www.abacom.de
 The pcb outline is 100 x 50 mm (width x height), all bitmaps have a resolution of 600dpi.
 Use FR-4 single sided photoresist epoxy pcb material for best results.

 (*) When printing the layout, be sure to resize it!

 (c)2005 RDVV. The Netherlands
 Rework (C)2006 Harm (Helix Inc.). The Netherlands.

