 Note:
 ====

 The layout of the 10mW-8W(Profline) RF-amplifier has been created with sPRINT
 Layout v3.0. You can get a Shareware copy at: http://www.abacom.de
 The pcb outline is 111 x 37 mm (width x height), bitmap resolution is 600dpi.
 Use FR-4 single sided photoresist epoxy pcb material for best results.
 
 (*) When printing the layout, be sure to resize it!

 (c)2005 Helix Inc. The Netherlands.

