 Note:
 ====

 
 The layout of the BLX15 150 Watts NoTune FM broadcast (87,5-108MHz) RF-amplifier has been 
 created with sPRINT Layout v3.0. You can get a Shareware copy at: http://www.abacom.de
 The pcb outline is 200 x 50 mm (width x height), bitmap resolution is 600dpi.
 Use FR-4 double sided photoresist epoxy pcb material for best results.

 (*) When printing the layout, be sure to resize it!

 Rework (C)2006 Helix Inc., The Netherlands.
 (C)2005 Rdvv, The Netherlands.
 Original stripline calculations and design (C)1987 A.Q. Vlaanderen, The Netherlands.

 (That should cover it!)

