 Note:
 ====

 The layout of the BLF278  300Watts FM-broadcast (87.5-108MHz) broadband RF-amplifier has
 been created with sPRINT Layout v3.0.
 You can get a Shareware copy of sPRINT Layout at: http://www.abacom.de 
 The pcb outline is 178 x 61 mm (width x height), bitmap resolution is 600dpi.
 Use FR-4 (double) sided photoresist epoxy pcb material for best results.

 (*) When printing the layout, be sure to resize it!

 (C)2006 Helix Inc. The Netherlands.

