 Note:
 ====

 The layout of the 2SC1971 8 Watts FM broadcast (87,5-108MHz) broadband microstripline 
 RF-amplifier has been created with sPRINT Layout v3.0.
 You can get a Shareware copy at: http://www.abacom.de
 The pcb outline is 77 x 56 mm (width x height), bitmap resolution is 600dpi.
 Use FR-4 double sided photoresist epoxy pcb material for best results.

 (*) When printing the layout, be sure to resize it!

 Original design & documentation (C) ASPiSYS, Greece.
 Redone artwork e.t.c. (C)2005 Helix Inc. The Netherlands.

