 Note:
 ====

 The layout of the 5 Watts FM-broadcast transmitter 'Stentor' has been created with 
 sPRINT Layout v3.0. You can get a Shareware copy at: http://www.abacom.de
 The pcb outline is 137 x 46 mm (width x height), bitmap resolution is 600dpi.
 Use FR-4 single sided photoresist epoxy pcb material for best results.

 (*) When printing the layout, be sure to resize it!

 (C)2006 Helix Inc. The Netherlands.

