 Note:
 -----

 The layout of the BGY33C 20 Watts FM broadcast (87,5-108MHz) broadband RF-amplifier 
 (revision 2) has been created with sPRINT Layout v3.0.
 You can get a Shareware copy at: http://www.abacom.de
 The pcb outline is: 160 x 34 mm (width x height), bitmap resolution is 600dpi.
 Use FR-4 single/double sided photoresist epoxy pcb material for best results.
 
 (*) When printing the layout, be sure to resize it! 

 Original design without rf-power adjustment by (c)Unique Electronics. Germany.
 (c)2005 Helix Inc. The Netherlands.

