 Note:
 -----

 The layout of the BFR91-BFR96(S)-2SC1971 6 Watts FM broadcast (87,5-108MHz) Profline 
 Broadband RF-amplifier has been created with sPRINT Layout v3.0.
 You can get a Shareware copy at: http://www.abacom.de
 The pcb outline is: 85 x 55 mm (width x height), bitmap resolution is 600dpi.
 Use FR-4 double sided photoresist epoxy pcb material for best results.
 
 (*) When printing the layout, be sure to resize it! 

 Design (C)2005 Rdvv, The Netherlands.
 Rework (C)2006 by Helix. The Netherlands.
 Intitial 2SC1971 microstripline design (C)2002 Sotiris Papadimitriou/ASPiSYS, Ltd. Greece.
 (That should cover it!)

 URL  : http://groups.yahoo.com/group/lpfm-pirate_radio/
 email: tri0de@hotmail.com

 NOT TO BE USED FOR COMMERCIAL PURPOSES!

