 Note:
 ====

 
 The layout of the BLW60C 50 Watts FM broadcast (87,5-108MHz) RF-amplifier has been created 
 with sPRINT Layout v3.0 You can get a Shareware copy at: http://www.abacom.de
 The pcb outline is 120 x 74 mm (width x height), bitmap resolution is 600dpi.
 Use FR-4 double sided photoresist epoxy pcb material for best results.

 (*) When printing the layout, be sure to resize it!

 (c)2005 Helix Inc. The Netherlands.

