 Note:
 ====

 The layout of the 300 mWatts FM-broadcast transmitter has been created with sPRINT
 Layout v3.0. You can get a Shareware copy at: http://www.abacom.de
 The pcb outline is 108 x 72 mm (width x height), bitmap resolution is 600dpi.
 Use FR-4 single sided photoresist epoxy pcb material for best results.

 (*) When printing the layout, be sure to resize it!

 (c)2005 Helix Inc. The Netherlands.

