 Note:
 ====

 The layout of the 150 Watts BLF177 FM broadcast (87,5-108MHz) RF-broadband amplifier has
 been created with sPRINT Layout v3.0.
 You can get a Shareware copy at: http://www.abacom.de 
 The pcb outline is 155 x 100 mm (width x height), bitmap resolution is 600dpi.
 Use FR-4 double sided photoresist epoxy pcb material for best results.

 (*) When printing the layout, be sure to resize it!

 (c)2005 Helix Inc. The Netherlands.

