 Note:
 ====

 The layout of the ERDS v1.1 RDS-Encoder has been created with sPRINT Layout v3.0. You can 
 get a Shareware copy at: http://www.abacom.de
 The pcb outline is 100 x 60 mm (width x height), bitmap resolution is 600dpi.
 Use FR-4 single sided photoresist epoxy pcb material for best results.

 (*) When printing the layout, be sure to resize it!

 Artwork (C)2005 Helix Inc. The Netherlands.

