 Note:
 ====

 The layout of the 1,5 Watts FM-broadcast transmitter has been created with sPRINT
 Layout v3.0. You can get a Shareware copy at: http://www.abacom.de
 The pcb outline is 146 x 72 mm (width x height), bitmaps have a resolution of 600dpi.
 Use FR-4 single sided photoresist epoxy pcb material for best results.

 (*) When printing the layout, be sure to resize it!


 You can contact me at: batterijbuis@hotmail.com

 
 (C)2006-2007 Lorian, The Netherlands.

 THIS DESIGN IS *NOT* TO BE USED FOR COMMERCIAL PURPOSES!

 (Sunday, January 14, 2007 (rev.3))

